IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and ARCHICAD 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: Off]"
Description: "Option [Export geometries that Participates in Collision Detection only: Off]"
Description: "Option [Split complex elements: Off]"
Description: "Option [Material Preservation: Explode where necessary]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved]"
Description: "Option [IFC Model position: Survey Point and Project Origin]"
Description: "Option [Curtain Wall export mode: Single Element]"
Description: "Option [Railing export mode: Single Element]"
File name: "C:\Users\cna\Gruner AG\ESD [G_INT] - Docs - ESD interne Dokumente\04_Projekte\B_Q2_2022_Digitaler_WBW_Mobimo\03_Modell\IFC\01_Studie.ifc"
Time stamp: "2022-06-28T16:48:24"
Author: "Catunda Natasha"
Organization: "Gruner"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.09 : 26 Sep 2013"
Originating system: "IFC file generated by GRAPHISOFT ARCHICAD 25.0.0 CHE FULL Windows version (IFC add-on version: 5005 CHE FULL)."
Authorization: "Catunda Natasha"
Application: "ARCHICAD" version "25.0.0" identifier "IFC add-on version: 5005 CHE FULL" by Organization "GRAPHISOFT" id "GS" description "GRAPHISOFT"

People and organizations
  Person "Natasha" "Catunda" of Organization "Gruner"
  Owner history of Person "Natasha" "Catunda" of Organization "Gruner" | application "ARCHICAD" version "25.0.0" identifier "IFC add-on version: 5005 CHE FULL" by Organization "GRAPHISOFT" id "GS" description "GRAPHISOFT" | change NOCHANGE | created 1656427703 (2022-06-28T14:48:23Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: SQUAREDEGREE (conversion based)
  CURRENCY: CHF
  TIMEUNIT: Year (conversion based)
  MASSUNIT: KILO GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN
  ENERGYUNIT: MEGA JOULE
  THERMALCONDUCTANCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  MASSDENSITYUNIT: derived

Spatial structure
IFCPROJECT "Mobimo-Test" | description "Test für Digitaler Wettbewerb. Austausch-Information mit IFC"
  IFCSITE "OE6293" | latitude 46° 54′ 0″ | longitude 8° 15′ 0″ | elevation above sea level 473. | postal address: "Siewerdtstrasse 27", "Zürich", "8050", "Schweiz"
    IFCBUILDING "Machbarkeitsstudie" | postal address: "Siewerdtstrasse 27", "Zürich", "8050", "Schweiz"
      IFCBUILDINGSTOREY "UG" | elevation -2.85
        contains 20 elements
          5 x IFCWALL | type IFCWALLTYPE "Beton, Sichtbeton 500" | names: "Wand-002", "Wand-003", "Wand-004" (+2 more) | material: "Beton, Sichtbeton" | property sets: Pset_WallCommon, Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, BaseQuantities
          11 x IFCWALL | type IFCWALLTYPE "MW, Backstein 500" | names: "Wand-001", "Wand-002", "Wand-003" (+4 more) | material: "MW, Backstein" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          3 x IFCWALL | type IFCWALLTYPE "MW, Backstein 250" | names: "Wand-001", "Wand-002" | material: "MW, Backstein" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Beton, Stahlbeton 250" | BASESLAB | names: "Decke-001" | material: layers "Beton, Stahlbeton 0.25" ("Beton, Stahlbeton" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
      IFCBUILDINGSTOREY "EG" | elevation 0.
        contains 20 elements
          9 x IFCWALL | type IFCWALLTYPE "Beton, Stahlbeton 500" | names: "Wand-001", "Wand-002", "Wand-003" (+6 more) | material: "Beton, Stahlbeton" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          7 x IFCWALL | type IFCWALLTYPE "MW, Backstein 250" | names: "Wand-001", "Wand-002", "Wand-003" (+2 more) | material: "MW, Backstein" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "MW, Backstein 150" | names: "Wand-003" | material: "MW, Backstein" | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          3 x IFCSLAB | type IFCSLABTYPE "Beton, Stahlbeton 250" | FLOOR | names: "Decke-001" | material: layers "Beton, Stahlbeton 0.25" ("Beton, Stahlbeton" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
      IFCBUILDINGSTOREY "OG" | elevation 2.85
        contains 26 elements
          8 x IFCWALL | type IFCWALLTYPE "Beton, Stahlbeton 500" | names: "Wand-001", "Wand-002", "Wand-003" (+5 more) | material: "Beton, Stahlbeton" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "1-Flügelfenster 25" | names: "Fenster-001" | property sets: AC_Pset_RenovationAndPhasing, Pset_WindowCommon, BaseQuantities
          7 x IFCWALL | type IFCWALLTYPE "MW, Backstein 250" | names: "Wand-001", "Wand-002", "Wand-003" (+2 more) | material: "MW, Backstein" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "MW, Backstein 150" | names: "Wand-003" | material: "MW, Backstein" | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Blockfutter 25" | names: "Tür-001" | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Beton, Stahlbeton 250" | FLOOR | names: "Decke-001" | material: layers "Beton, Stahlbeton 0.25" ("Beton, Stahlbeton" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Leichtbau 1.5/10/1.5cm 130" | names: "Wand-001", "Wand-002" | descriptions: "Leichtbau" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Kunststein, Betonwerkstein 250" | FLOOR | names: "Decke-001" | material: layers "Kunststein, Betonwerkstein 0.25" ("Kunststein, Betonwerkstein" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
        IFCSPACE "01" | long name "WOHNEN" | INTERNAL
        IFCSPACE "01" | long name "WC" | INTERNAL
        IFCSPACE "02" | long name "Küche" | INTERNAL
        IFCSPACE "03" | long name "BALKON" | INTERNAL
      IFCBUILDINGSTOREY "OG" | elevation 5.7
        contains 26 elements
          8 x IFCWALL | type IFCWALLTYPE "Beton, Stahlbeton 500" | names: "Wand-001", "Wand-002", "Wand-003" (+5 more) | material: "Beton, Stahlbeton" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "1-Flügelfenster 25" | names: "Fenster-001" | property sets: AC_Pset_RenovationAndPhasing, Pset_WindowCommon, BaseQuantities
          7 x IFCWALL | type IFCWALLTYPE "MW, Backstein 250" | names: "Wand-001", "Wand-002", "Wand-003" (+2 more) | material: "MW, Backstein" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "MW, Backstein 150" | names: "Wand-003" | material: "MW, Backstein" | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Blockfutter 25" | names: "Tür-001" | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Beton, Stahlbeton 250" | FLOOR | names: "Decke-001" | material: layers "Beton, Stahlbeton 0.25" ("Beton, Stahlbeton" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Leichtbau 1.5/10/1.5cm 130" | names: "Wand-001", "Wand-002" | descriptions: "Leichtbau" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Kunststein, Betonwerkstein 250" | FLOOR | names: "Decke-001" | material: layers "Kunststein, Betonwerkstein 0.25" ("Kunststein, Betonwerkstein" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
      IFCBUILDINGSTOREY "OG" | elevation 8.55
        contains 26 elements
          8 x IFCWALL | type IFCWALLTYPE "Beton, Stahlbeton 500" | names: "Wand-001", "Wand-002", "Wand-003" (+5 more) | material: "Beton, Stahlbeton" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "1-Flügelfenster 25" | names: "Fenster-001" | property sets: AC_Pset_RenovationAndPhasing, Pset_WindowCommon, BaseQuantities
          7 x IFCWALL | type IFCWALLTYPE "MW, Backstein 250" | names: "Wand-001", "Wand-002", "Wand-003" (+2 more) | material: "MW, Backstein" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "MW, Backstein 150" | names: "Wand-003" | material: "MW, Backstein" | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Blockfutter 25" | names: "Tür-001" | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Beton, Stahlbeton 250" | FLOOR | names: "Decke-001" | material: layers "Beton, Stahlbeton 0.25" ("Beton, Stahlbeton" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Leichtbau 1.5/10/1.5cm 130" | names: "Wand-001", "Wand-002" | descriptions: "Leichtbau" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Kunststein, Betonwerkstein 250" | FLOOR | names: "Decke-001" | material: layers "Kunststein, Betonwerkstein 0.25" ("Kunststein, Betonwerkstein" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
      IFCBUILDINGSTOREY "OG" | elevation 11.4
        contains 27 elements
          8 x IFCWALL | type IFCWALLTYPE "Beton, Stahlbeton 500" | names: "Wand-001", "Wand-002", "Wand-003" (+5 more) | material: "Beton, Stahlbeton" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "1-Flügelfenster 25" | names: "Fenster-001" | property sets: AC_Pset_RenovationAndPhasing, Pset_WindowCommon, BaseQuantities
          7 x IFCWALL | type IFCWALLTYPE "MW, Backstein 250" | names: "Wand-001", "Wand-002", "Wand-003" (+2 more) | material: "MW, Backstein" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "Kunststein, Betonwerkstein 250" | FLOOR | names: "Decke-001" | material: layers "Kunststein, Betonwerkstein 0.25" ("Kunststein, Betonwerkstein" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "MW, Backstein 150" | names: "Wand-003" | material: "MW, Backstein" | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Blockfutter 25" | names: "Tür-001" | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Leichtbau 1.5/10/1.5cm 130" | names: "Wand-001", "Wand-002" | descriptions: "Leichtbau" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Beton, Stahlbeton 250" | FLOOR | names: "Decke-001" | material: layers "Beton, Stahlbeton 0.25" ("Beton, Stahlbeton" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
      IFCBUILDINGSTOREY "OG" | elevation 14.25
        contains 27 elements
          8 x IFCWALL | type IFCWALLTYPE "Beton, Stahlbeton 500" | names: "Wand-001", "Wand-002", "Wand-003" (+5 more) | material: "Beton, Stahlbeton" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "1-Flügelfenster 25" | names: "Fenster-001" | property sets: AC_Pset_RenovationAndPhasing, Pset_WindowCommon, BaseQuantities
          7 x IFCWALL | type IFCWALLTYPE "MW, Backstein 250" | names: "Wand-001", "Wand-002", "Wand-003" (+2 more) | material: "MW, Backstein" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "Kunststein, Betonwerkstein 250" | FLOOR | names: "Decke-001" | material: layers "Kunststein, Betonwerkstein 0.25" ("Kunststein, Betonwerkstein" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "MW, Backstein 150" | names: "Wand-003" | material: "MW, Backstein" | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Blockfutter 25" | names: "Tür-001" | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "Leichtbau 1.5/10/1.5cm 130" | names: "Wand-001", "Wand-002" | descriptions: "Leichtbau" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Beton, Stahlbeton 250" | FLOOR | names: "Decke-001" | material: layers "Beton, Stahlbeton 0.25" ("Beton, Stahlbeton" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
      IFCBUILDINGSTOREY "DG" | elevation 17.1
        contains 22 elements
          4 x IFCWALL | type IFCWALLTYPE "Beton, Stahlbeton 500" | names: "Wand-001", "Wand-004", "Wand-005" (+1 more) | material: "Beton, Stahlbeton" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          2 x IFCSLAB | type IFCSLABTYPE "Kunststein, Betonwerkstein 250" | FLOOR | names: "Decke-001" | material: layers "Kunststein, Betonwerkstein 0.25" ("Kunststein, Betonwerkstein" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
          7 x IFCWALL | type IFCWALLTYPE "MW, Backstein 250" | names: "Wand-001", "Wand-002", "Wand-003" (+2 more) | material: "MW, Backstein" | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "1-Flügelfenster 25" | names: "Fenster-001" | property sets: AC_Pset_RenovationAndPhasing, Pset_WindowCommon, BaseQuantities
          1 x IFCWALL | type IFCWALLTYPE "MW, Backstein 150" | names: "Wand-003" | material: "MW, Backstein" | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Blockfutter 25" | names: "Tür-001" | property sets: AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Beton, Stahlbeton 300" | ROOF | names: "Decke-001" | material: layers "Beton, Stahlbeton 0.3" ("Beton, Stahlbeton" 0.3) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Beton, Stahlbeton 250" | FLOOR | names: "Decke-001" | material: layers "Beton, Stahlbeton 0.25" ("Beton, Stahlbeton" 0.25) | property sets: Eigenschaften_Schweiz_Allgemein, AC_Pset_RenovationAndPhasing, Pset_SlabCommon, BaseQuantities

Types
  IFCWALLTYPE "Beton, Sichtbeton 500" | 5 occurrences
  IFCWALLTYPE "MW, Backstein 500" | 11 occurrences
  IFCWALLTYPE "MW, Backstein 250" | 52 occurrences
  IFCSLABTYPE "Beton, Stahlbeton 250" | BASESLAB | 1 occurrence
  IFCWALLTYPE "Beton, Stahlbeton 500" | 53 occurrences
  IFCWALLTYPE "MW, Backstein 150" | 7 occurrences
  IFCSLABTYPE "Beton, Stahlbeton 250" | FLOOR | 9 occurrences
  IFCWINDOWSTYLE "1-Flügelfenster 25" | SINGLE_PANEL | 30 occurrences
  IFCDOORSTYLE "Blockfutter 25" | SINGLE_SWING_RIGHT | 6 occurrences
  IFCWALLTYPE "Leichtbau 1.5/10/1.5cm 130" | 10 occurrences
  IFCSLABTYPE "Kunststein, Betonwerkstein 250" | FLOOR | 9 occurrences
  IFCSLABTYPE "Beton, Stahlbeton 300" | ROOF | 1 occurrence

Property sets
  BaseQuantities | quantities | on 15 objects (15 IFCOPENINGELEMENT)
    Area = 4.3039999994 [SQUARE_METRE]
    Depth = 0.5 [METRE]
    Height = 2.69 [METRE]
    Volume = 0.133732085506 [CUBIC_METRE]
    Width = 1.59999999963 [METRE]
  BaseQuantities | quantities | on 15 objects (15 IFCWINDOW)
    Area = 4.3039999994 [SQUARE_METRE]
    Depth = 0.5 [METRE]
    GrossArea = 4.3039999994 [SQUARE_METRE]
    Height = 2.69 [METRE]
    NetVolume = 0.133732085506 [CUBIC_METRE]
    Perimeter = 8.57999999925 [METRE]
    Volume = 0.133732085506 [CUBIC_METRE]
    Width = 1.59999999963 [METRE]
  BaseQuantities | quantities | on 7 objects (7 IFCBUILDINGSTOREY)
    GrossFloorArea = 0. [SQUARE_METRE]
    GrossHeight = 2.85 [METRE]
    Height = 2.85 [METRE]
    NetHeight = 2.85 [METRE]
  BaseQuantities | quantities | on 7 objects (7 IFCOPENINGELEMENT)
    Area = 4.3039999994 [SQUARE_METRE]
    Depth = 0.5 [METRE]
    Height = 2.69 [METRE]
    Volume = 0.133732085506 [CUBIC_METRE]
    Width = 1.60000000009 [METRE]
  BaseQuantities | quantities | on 7 objects (7 IFCWINDOW)
    Area = 4.3039999994 [SQUARE_METRE]
    Depth = 0.5 [METRE]
    GrossArea = 4.3039999994 [SQUARE_METRE]
    Height = 2.69 [METRE]
    NetVolume = 0.133732085506 [CUBIC_METRE]
    Perimeter = 8.58000000019 [METRE]
    Volume = 0.133732085506 [CUBIC_METRE]
    Width = 1.60000000009 [METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCWALL)
    GrossFootprintArea = 1.10841719143 [SQUARE_METRE]
    GrossSideArea = 11.5275387865 [SQUARE_METRE]
    GrossVolume = 2.88188469756 [CUBIC_METRE]
    Height = 2.6 [METRE]
    Length = 4.30866876493 [METRE]
    NetFootprintArea = 1.10841719143 [SQUARE_METRE]
    NetSideArea = 11.5275387865 [SQUARE_METRE]
    NetVolume = 2.88188469756 [CUBIC_METRE]
    Width = 0.25 [METRE]
  BaseQuantities | quantities | on 5 objects (5 IFCWALL)
    GrossFootprintArea = 1.48845558893 [SQUARE_METRE]
    GrossSideArea = 15.4799381257 [SQUARE_METRE]
    GrossVolume = 3.86998453456 [CUBIC_METRE]
    Height = 2.6 [METRE]
    Length = 6.10382235171 [METRE]
    NetFootprintArea = 1.48845558893 [SQUARE_METRE]
    NetSideArea = 15.4799381257 [SQUARE_METRE]
    NetVolume = 3.86998453456 [CUBIC_METRE]
    Width = 0.25 [METRE]
  BaseQuantities | quantities | on 5 objects (5 IFCWALL)
    GrossFootprintArea = 2.90800247249 [SQUARE_METRE]
    GrossSideArea = 15.1216128701 [SQUARE_METRE]
    GrossVolume = 7.56080643419 [CUBIC_METRE]
    Height = 2.6 [METRE]
    Length = 6.31600505012 [METRE]
    NetFootprintArea = 2.90800247249 [SQUARE_METRE]
    NetSideArea = 15.1216128701 [SQUARE_METRE]
    NetVolume = 7.56080643419 [CUBIC_METRE]
    Width = 0.5 [METRE]
  BaseQuantities: 122 more contents on 187 objects not shown
  Pset_WallCommon | properties | on 67 objects (67 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 53 objects (53 IFCWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 10 objects (10 IFCWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 5 objects (5 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    Compartmentation = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
  Eigenschaften_Schweiz_Allgemein | properties | on 112 objects (112 IFCWALL)
    Unter Terrain = FALSE (IFCBOOLEAN)
  Eigenschaften_Schweiz_Allgemein | properties | on 11 objects (11 IFCWALL)
    Aussenliegendes Bauteil = FALSE (IFCBOOLEAN)
    Schutzschicht = FALSE (IFCBOOLEAN)
    Unter Terrain = TRUE (IFCBOOLEAN)
  Eigenschaften_Schweiz_Allgemein | properties | on 9 objects (9 IFCSLAB)
    Balkon = TRUE (IFCBOOLEAN)
  Eigenschaften_Schweiz_Allgemein | properties | on 7 objects (7 IFCSLAB)
    Balkon = FALSE (IFCBOOLEAN)
  Eigenschaften_Schweiz_Allgemein | properties | on 5 objects (5 IFCWALL)
    Aussenliegendes Bauteil = TRUE (IFCBOOLEAN)
    Konstruktionsergänzung = "Abdichtung" (IFCLABEL)
    Schutzschicht = TRUE (IFCBOOLEAN)
    Unter Terrain = TRUE (IFCBOOLEAN)
  Eigenschaften_Schweiz_Allgemein | properties | on 3 objects (3 IFCWALL)
    Unter Terrain = TRUE (IFCBOOLEAN)
  Eigenschaften_Schweiz_Allgemein | properties | on 2 objects (2 IFCSLAB)
    Aussenliegendes Bauteil = TRUE (IFCBOOLEAN)
    Balkon = FALSE (IFCBOOLEAN)
  Eigenschaften_Schweiz_Allgemein | properties | on 1 object (1 IFCSLAB)
    Aussenliegendes Bauteil = TRUE (IFCBOOLEAN)
  Eigenschaften_Schweiz_Allgemein: 1 more content on 1 objects not shown
  AC_Pset_RenovationAndPhasing | properties | on 151 objects (129 IFCWALL, 16 IFCSLAB, 6 IFCDOOR)
    Renovation Status = "New" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 57 objects (30 IFCWINDOW, 10 IFCOPENINGELEMENT, 9 IFCWALL, 4 IFCSLAB)
    Renovation Status = "Existing" (IFCLABEL)
  Pset_SlabCommon | properties | on 13 objects (13 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_SlabCommon | properties | on 7 objects (7 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 30 objects (30 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_SpaceCommon | properties | on 3 objects (3 IFCSPACE)
    Category = "HNF" (IFCLABEL)
    Reference = "HNF" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "ANF" (IFCLABEL)
    Reference = "ANF" (IFCIDENTIFIER)