IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [ContentGUID: 813b09a7-4544-472a-a2ec-350355f9d09a, VersionGUID: 71e5c979-308f-40c9-ab28-790243b83879, NumberOfSaves: 43]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates, ProjectSite: Default Site]"
File name: "P24-142 v_2024_11_26.ifc"
Time stamp: "2024-11-26T17:06:16+00:00"
Preprocessor: "ODA SDAI 24.12"
Originating system: "Autodesk Revit 25.3.0.46 (ENG) - IFC 25.3.0.46"
Application: "Autodesk Revit 2025 (ENG)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ENG)"

People and organizations
  Person "and.magro" of Organization "várias"
  Owner history of Person "and.magro" of Organization "várias" | application "Autodesk Revit 2025 (ENG)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ENG)" | change NOCHANGE | created 1732613468 (2024-11-26T09:31:08Z)

Units
  LENGTHUNIT: METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  AREAUNIT: SQUARE_METRE
  THERMALTRANSMITTANCEUNIT: derived

Spatial structure
IFCPROJECT | long name "Estabilidade" | phase "Projeto de Execução"
  IFCSITE "Default" | latitude 42° 21′ 31.401672″ | longitude -71° 3′ 24.318237″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Boston", "MA"
      IFCBUILDINGSTOREY "Piso 0 IFC" | long name "Piso 0 IFC" | object type "Level:8mm Head" | elevation 0.
        contains 112 elements
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1162688" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1163030" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1163135" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1163690", "H-Wide Flange-Column:HE120B:1163981", "H-Wide Flange-Column:HE120B:1164222" (+3 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1164493", "H-Wide Flange-Column:HE120B:1164766", "H-Wide Flange-Column:HE120B:1164848" (+3 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1165256", "H-Wide Flange-Column:HE120B:1166175", "H-Wide Flange-Column:HE120B:1166340" (+1 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1168683" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1168738" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1168860" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1169025" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1169204" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1170341" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1170342" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          21 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:20 cm" | object type "Basic Wall:20 cm" | names: "Basic Wall:20 cm:1170767", "Basic Wall:20 cm:1171351", "Basic Wall:20 cm:1171449" (+18 more) | material: layers "Basic Wall:20 cm" ("Betão armado C25/30" 0.20000000000000001) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCWALL | type IFCWALLTYPE "Basic Wall:20 cm" | object type "Basic Wall:20 cm" | names: "Basic Wall:20 cm:1172273", "Basic Wall:20 cm:1245422" | material: layers "Basic Wall:20 cm" ("Betão armado C25/30" 0.20000000000000001) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1177817" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1178645" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1178808" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1178910" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1179040" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1179187" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          2 x IFCSLAB | type IFCSLABTYPE "Floor:Generic 200mm" | object type "Floor:Generic 200mm" | FLOOR | names: "Floor:Generic 200mm:1179586", "Floor:Generic 200mm:1236090" | material: layers "Floor:Generic 200mm" ("Betão armado C25/30" 0.20000000000000001) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 400mm" | object type "Floor:Generic Floor - 400mm" | FLOOR | names: "Floor:Generic Floor - 400mm:1180419" | material: layers "Floor:Generic Floor - 400mm" ("Default Floor" 0.40000000000000002) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:300mm" | object type "Concrete Round:300mm" | names: "Concrete Round:300mm:1181943" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:300mm" | object type "Concrete Round:300mm" | names: "Concrete Round:300mm:1182045" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:300mm" | object type "Concrete Round:300mm" | names: "Concrete Round:300mm:1182183" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:300mm" | object type "Concrete Round:300mm" | names: "Concrete Round:300mm:1182239" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:300mm" | object type "Concrete Round:300mm" | names: "Concrete Round:300mm:1182330" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:25 x 20cm" | object type "M_Concrete-Rectangular-Column:25 x 20cm" | names: "M_Concrete-Rectangular-Column:25 x 20cm:1182881" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:escadas de acesso ao passadiço 2" | object type "Assembled Stair:escadas de acesso ao passadiço 2" | STRAIGHT_RUN_STAIR | names: "Assembled Stair:Stair:1191719" | parts: 2 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCBEAM | type IFCBEAMTYPE "U-Channels:UPN80" | object type "U-Channels:UPN80" | names: "U-Channels:UPN80:1199719" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Curtain Wall" | object type "Curtain Wall:Curtain Wall" | names: "Curtain Wall:Curtain Wall:1232453" | parts: 39 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:15 cm" | object type "Basic Wall:15 cm" | names: "Basic Wall:15 cm:1234514", "Basic Wall:15 cm:1235546", "Basic Wall:15 cm:1235634" | material: layers "Basic Wall:15 cm" ("Betão armado C25/30" 0.14999999999999997) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Generic - 400mm" | object type "Basic Wall:Generic - 400mm" | names: "Basic Wall:Generic - 400mm:1239011" | material: layers "Basic Wall:Generic - 400mm" ("Parede Branca" 0.40000000000000002) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCMEMBER | type IFCMEMBERTYPE "U-Channels:UPN100" | object type "U-Channels:UPN100" | names: "U-Channels:UPN100:1247336" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "U-Channels:UPN80" | object type "U-Channels:UPN80" | names: "U-Channels:UPN80:1255792" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "U-Channels:UPN80" | object type "U-Channels:UPN80" | names: "U-Channels:UPN80:1255936" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1256870" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257423" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257472" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257654" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257655" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "U-Channels:UPN100" | object type "U-Channels:UPN100" | names: "U-Channels:UPN100:1257756" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257966", "L-Angles:CAE50x5:1258205" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258283", "L-Angles:CAE50x5:1258450" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258329", "L-Angles:CAE50x5:1258451" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Foundation Slab:200mm Foundation Slab" | object type "Foundation Slab:200mm Foundation Slab" | BASESLAB | names: "Foundation Slab:200mm Foundation Slab:1258584" | material: layers "Foundation Slab:200mm Foundation Slab" ("Concrete, Cast-in-Place gray" 0.20000000000000001) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | object type "M_Concrete-Rectangular-Column:44 x 44 cm" | names: "M_Concrete-Rectangular-Column:44 x 44 cm:1262932" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 2:Generic Models 2" | object type "Generic Models 2:Generic Models 2" | names: "Generic Models 2:Generic Models 2:1269690" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1274820" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1274901" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1275161" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1275472" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          2 x IFCSLAB | type IFCSLABTYPE "Foundation Slab:300mm Foundation Slab" | object type "Foundation Slab:300mm Foundation Slab" | BASESLAB | names: "Foundation Slab:300mm Foundation Slab:1277325", "Foundation Slab:300mm Foundation Slab:1277325:2" | material: layers "Foundation Slab:300mm Foundation Slab" ("Concrete, Cast-in-Place gray" 0.30000000000000004) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:600mm Arial" | object type "Model Text:600mm Arial" | names: "Model Text:600mm Arial:1277581", "Model Text:600mm Arial:1283029", "Model Text:600mm Arial:1283037" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1311430" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1312654" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1313163" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1313464" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1313501" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Concrete Round:360mm" | object type "Concrete Round:360mm" | names: "Concrete Round:360mm:1313565" | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IPE-Column:IPE200" | object type "IPE-Column:IPE200" | names: "IPE-Column:IPE200:1318677" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IPE-Column:IPE200" | object type "IPE-Column:IPE200" | names: "IPE-Column:IPE200:1318933" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IPE-Column:IPE200" | object type "IPE-Column:IPE200" | names: "IPE-Column:IPE200:1319115" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Default" | object type "Pipe Types:Default" | names: "Pipe Types:Default:1328613" | property sets: Pset_DistributionFlowElementCommon, Pset_DuctConnection, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_PipeConnection, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Elbow - Welded - Generic:Standard" | object type "M_Elbow - Welded - Generic:Standard" | names: "M_Elbow - Welded - Generic:Standard:1328636", "M_Elbow - Welded - Generic:Standard:1329267" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_PipeFittingTypeCommon, Pset_QuantityTakeOff
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Standard" | object type "Pipe Types:Standard" | names: "Pipe Types:Standard:1329167" | property sets: Pset_DistributionFlowElementCommon, Pset_DuctConnection, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_PipeConnection, Pset_QuantityTakeOff
          1 x IFCBEAM | type IFCBEAMTYPE "IPE-Beams:IPE120" | object type "IPE-Beams:IPE120" | names: "IPE-Beams:IPE120:1331648" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
      IFCBUILDINGSTOREY "Piso 0.1" | long name "Piso 0.1" | object type "Level:8mm Head" | elevation 2.4999999999999996
        contains 50 elements
          8 x IFCBEAM | type IFCBEAMTYPE "H-Wide Flange Beams:HE120B" | object type "H-Wide Flange Beams:HE120B" | names: "H-Wide Flange Beams:HE120B:1167891", "H-Wide Flange Beams:HE120B:1167929", "H-Wide Flange Beams:HE120B:1167960" (+5 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          13 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1186601", "L-Angles:CAE80x8:1187660", "L-Angles:CAE80x8:1188004" (+10 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1186627" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1186654" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1186672" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1186914" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          3 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1186915", "L-Angles:CAE80x8:1187688", "L-Angles:CAE80x8:1188005" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1186916" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1186917" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1187986" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1187987" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1190160", "L-Angles:CAE80x8:1190258" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1190274" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1190275" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257343" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257346" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257675" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257676" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          3 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258208", "L-Angles:CAE50x5:1258211", "L-Angles:CAE50x5:1258214" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258481", "L-Angles:CAE50x5:1258484" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258482", "L-Angles:CAE50x5:1258485" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Mass 3:Mass 3" | object type "Mass 3:Mass 3" | names: "Mass 3:Mass 3:1277870" | material: "Default Form" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:600mm Arial" | object type "Model Text:600mm Arial" | names: "Model Text:600mm Arial:1277872" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1312881" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
      IFCBUILDINGSTOREY "Piso 1" | long name "Piso 1" | object type "Level:8mm Head" | elevation 3.8999999999999999
        contains 106 elements
          14 x IFCBEAM | type IFCBEAMTYPE "H-Wide Flange Beams:HE120B" | object type "H-Wide Flange Beams:HE120B" | names: "H-Wide Flange Beams:HE120B:1167367", "H-Wide Flange Beams:HE120B:1167431", "H-Wide Flange Beams:HE120B:1167476" (+11 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          9 x IFCBEAM | type IFCBEAMTYPE "H-Wide Flange Beams:HE120B" | object type "H-Wide Flange Beams:HE120B" | names: "H-Wide Flange Beams:HE120B:1176238", "H-Wide Flange Beams:HE120B:1176269", "H-Wide Flange Beams:HE120B:1176405" (+6 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCMEMBER | type IFCMEMBERTYPE "H-Wide Flange Beams:HE120B" | object type "H-Wide Flange Beams:HE120B" | names: "H-Wide Flange Beams:HE120B:1176438", "H-Wide Flange Beams:HE120B:1176466" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCBEAM | type IFCBEAMTYPE "U-Channels:UPN100" | object type "U-Channels:UPN100" | names: "U-Channels:UPN100:1188681", "U-Channels:UPN100:1193658" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "U-Channels:UPN100" | object type "U-Channels:UPN100" | names: "U-Channels:UPN100:1189107", "U-Channels:UPN100:1189466" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Gradil 50mm" | object type "Floor:Gradil 50mm" | FLOOR | names: "Floor:Gradil 50mm:1190319" | material: layers "Floor:Gradil 50mm" ("Betão armado C25/30" 0.050000000000000003) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          12 x IFCBEAM | type IFCBEAMTYPE "U-Channels:UPN80" | object type "U-Channels:UPN80" | names: "U-Channels:UPN80:1199381", "U-Channels:UPN80:1199659", "U-Channels:UPN80:1203311" (+9 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          7 x IFCMEMBER | type IFCMEMBERTYPE "U-Channels:UPN80" | object type "U-Channels:UPN80" | names: "U-Channels:UPN80:1200614", "U-Channels:UPN80:1200722", "U-Channels:UPN80:1200820" (+4 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          3 x IFCMEMBER | type IFCMEMBERTYPE "U-Channels:UPN80" | object type "U-Channels:UPN80" | names: "U-Channels:UPN80:1201428", "U-Channels:UPN80:1201491", "U-Channels:UPN80:1201566" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCMEMBER | type IFCMEMBERTYPE "U-Channels:UPN160" | object type "U-Channels:UPN160" | names: "U-Channels:UPN160:1201666", "U-Channels:UPN160:1201667" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Condensadores:Condensadores" | object type "Condensadores:Condensadores" | names: "Condensadores:Condensadores:1202776" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Condensadores1:Condensadores" | object type "Condensadores1:Condensadores" | names: "Condensadores1:Condensadores:1202857" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "U-Channels:UPN80" | object type "U-Channels:UPN80" | names: "U-Channels:UPN80:1203436" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1205124" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1205177" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1205411" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:60 mm" | object type "Model Text:60 mm" | names: "Model Text:60 mm:1207823", "Model Text:60 mm:1207833" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCSTAIR | type IFCTYPEPRODUCT "Assembled Stair:escadas de acesso ao passadiço 2" | object type "Assembled Stair:escadas de acesso ao passadiço 2" | STRAIGHT_RUN_STAIR | names: "Assembled Stair:Stair:1212097" | parts: 2 IFCRAILING, 1 IFCSTAIRFLIGHT | property sets: Pset_QuantityTakeOff, Pset_StairCommon
          1 x IFCBEAM | type IFCBEAMTYPE "U-Channels:UPN80" | object type "U-Channels:UPN80" | names: "U-Channels:UPN80:1212633" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257349" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257352" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257678" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257679" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258217", "L-Angles:CAE50x5:1258220" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258487" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258488" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Coberto Nova Parede:Coberto Nova Parede" | object type "Coberto Nova Parede:Coberto Nova Parede" | names: "Coberto Nova Parede:Coberto Nova Parede:1277004" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 3:Generic Models 3" | object type "Generic Models 3:Generic Models 3" | names: "Generic Models 3:Generic Models 3:1280105" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1297369", "H-Wide Flange-Column:HE120B:1298093", "H-Wide Flange-Column:HE120B:1300184" (+3 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1301942" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1302041" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1302136" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1302157" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1308569" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1313429" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1317738" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1317836" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1318009" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1318019" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1318031" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | object type "H-Wide Flange-Column:HE120B" | names: "H-Wide Flange-Column:HE120B:1318040" | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfColumn
          5 x IFCBEAM | type IFCBEAMTYPE "IPE-Beams:IPE120" | object type "IPE-Beams:IPE120" | names: "IPE-Beams:IPE120:1322251", "IPE-Beams:IPE120:1322375", "IPE-Beams:IPE120:1323130" (+2 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1323024" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1323075" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1323495" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1323544" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCBEAM | type IFCBEAMTYPE "IPE-Beams:IPE120" | object type "IPE-Beams:IPE120" | names: "IPE-Beams:IPE120:1323632" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1324670" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1324746" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1325322" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1325369" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Piso 2" | long name "Piso 2" | object type "Level:8mm Head" | elevation 4.9000000000000004
        contains 33 elements
          11 x IFCBEAM | type IFCBEAMTYPE "U-Channels:UPN80" | object type "U-Channels:UPN80" | names: "U-Channels:UPN80:1207900", "U-Channels:UPN80:1208035", "U-Channels:UPN80:1210684" (+8 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "U-Channels:UPN60" | object type "U-Channels:UPN60" | names: "U-Channels:UPN60:1215046", "U-Channels:UPN60:1215170" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257355" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257358" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257361" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257681" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257682" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          3 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258223", "L-Angles:CAE50x5:1258226", "L-Angles:CAE50x5:1258229" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258490" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258491" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Gradil 50mm" | object type "Floor:Gradil 50mm" | FLOOR | names: "Floor:Gradil 50mm:1258988" | material: layers "Floor:Gradil 50mm" ("Betão armado C25/30" 0.050000000000000003) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:600mm Arial" | object type "Model Text:600mm Arial" | names: "Model Text:600mm Arial:1259141" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1:Generic Models 1" | object type "Generic Models 1:Generic Models 1" | names: "Generic Models 1:Generic Models 1:1268670" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Coletor Principal Retorno v1:Coletor Principal Retorno v1" | object type "Coletor Principal Retorno v1:Coletor Principal Retorno v1" | names: "Coletor Principal Retorno v1:Coletor Principal Retorno v1:1282970" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Coletor Principal Envio:Coletor Principal Envio" | object type "Coletor Principal Envio:Coletor Principal Envio" | names: "Coletor Principal Envio:Coletor Principal Envio:1282990" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Mass 4:Mass 4" | object type "Mass 4:Mass 4" | names: "Mass 4:Mass 4:1291801" | material: "Default Form" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "IPE-Beams:IPE80" | object type "IPE-Beams:IPE80" | names: "IPE-Beams:IPE80:1302306" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "IPE-Beams:IPE80" | object type "IPE-Beams:IPE80" | names: "IPE-Beams:IPE80:1302749" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1323374" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE80x8" | object type "L-Angles:CAE80x8" | names: "L-Angles:CAE80x8:1323402" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Coberto 1" | long name "Coberto 1" | object type "Level:8mm Head" | elevation 6.9999999999999991
        contains 24 elements
          7 x IFCBEAM | type IFCBEAMTYPE "IPE-Beams:IPE100" | object type "IPE-Beams:IPE100" | names: "IPE-Beams:IPE100:1284884", "IPE-Beams:IPE100:1284919", "IPE-Beams:IPE100:1285657" (+4 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          4 x IFCBEAM | type IFCBEAMTYPE "U-Channels:UPN100" | object type "U-Channels:UPN100" | names: "U-Channels:UPN100:1284945", "U-Channels:UPN100:1284994", "U-Channels:UPN100:1303849" (+1 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Mass 5:Mass 5" | object type "Mass 5:Mass 5" | names: "Mass 5:Mass 5:1293638" | material: "Default Form" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Mass 7:Mass 7" | object type "Mass 7:Mass 7" | names: "Mass 7:Mass 7:1311122" | material: "Default Form" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:600mm Arial" | object type "Model Text:600mm Arial" | names: "Model Text:600mm Arial:1311149", "Model Text:600mm Arial:1311186" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "IPE-Beams:IPE80" | object type "IPE-Beams:IPE80" | names: "IPE-Beams:IPE80:1325016" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "IPE-Beams:IPE80" | object type "IPE-Beams:IPE80" | names: "IPE-Beams:IPE80:1325139" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "IPE-Beams:IPE80" | object type "IPE-Beams:IPE80" | names: "IPE-Beams:IPE80:1325186" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          4 x IFCBEAM | type IFCBEAMTYPE "IPE-Beams:IPE120" | object type "IPE-Beams:IPE120" | names: "IPE-Beams:IPE120:1331185", "IPE-Beams:IPE120:1331568", "IPE-Beams:IPE120:1331843" (+1 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Beam System:Structural Framing System:1284791", "Structural Beam System:Structural Framing System:1324850" | parts: 9 IFCBEAM | property sets: Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Coberto 2" | long name "Coberto 2" | object type "Level:8mm Head" | elevation 8.0952000000000002
        contains 26 elements
          2 x IFCBEAM | type IFCBEAMTYPE "IPE-Beams:IPE100" | object type "IPE-Beams:IPE100" | names: "IPE-Beams:IPE100:1301276", "IPE-Beams:IPE100:1302868" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          3 x IFCBEAM | type IFCBEAMTYPE "H-Wide Flange Beams:HE120B" | object type "H-Wide Flange Beams:HE120B" | names: "H-Wide Flange Beams:HE120B:1305943", "H-Wide Flange Beams:HE120B:1305983", "H-Wide Flange Beams:HE120B:1311977" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          4 x IFCBEAM | type IFCBEAMTYPE "H-Wide Flange Beams:HE120B" | object type "H-Wide Flange Beams:HE120B" | names: "H-Wide Flange Beams:HE120B:1306060", "H-Wide Flange Beams:HE120B:1306099", "H-Wide Flange Beams:HE120B:1312157" (+1 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "U-Channels:UPN120" | object type "U-Channels:UPN120" | names: "U-Channels:UPN120:1317006", "U-Channels:UPN120:1317054" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          3 x IFCMEMBER | type IFCMEMBERTYPE "IPE-Beams:IPE120" | object type "IPE-Beams:IPE120" | names: "IPE-Beams:IPE120:1317196", "IPE-Beams:IPE120:1317357", "IPE-Beams:IPE120:1322654" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          3 x IFCBEAM | type IFCBEAMTYPE "IPE-Beams:IPE120" | object type "IPE-Beams:IPE120" | names: "IPE-Beams:IPE120:1317272", "IPE-Beams:IPE120:1322826", "IPE-Beams:IPE120:1325589" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCMEMBER | type IFCMEMBERTYPE "IPE-Beams:IPE80" | object type "IPE-Beams:IPE80" | names: "IPE-Beams:IPE80:1324954" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCBEAM | type IFCBEAMTYPE "IPE-Beams:IPE120" | object type "IPE-Beams:IPE120" | names: "IPE-Beams:IPE120:1325565" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          4 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Pipe Types:Standard" | object type "Pipe Types:Standard" | names: "Pipe Types:Standard:1329255", "Pipe Types:Standard:1329401", "Pipe Types:Standard:1329444" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_DuctConnection, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_PipeConnection, Pset_QuantityTakeOff
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "M_Elbow - Welded - Generic:Standard" | object type "M_Elbow - Welded - Generic:Standard" | names: "M_Elbow - Welded - Generic:Standard:1329409", "M_Elbow - Welded - Generic:Standard:1329452", "M_Elbow - Welded - Generic:Standard:1329460" | material: "<Unnamed>" | property sets: Pset_DistributionFlowElementCommon, Pset_PipeFittingTypeCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Piso 2.3" | long name "Piso 2.3" | object type "Level:8mm Head" | elevation 8.8000000000000007
        contains 48 elements
          2 x IFCBEAM | type IFCBEAMTYPE "H-Wide Flange Beams:HE100B" | object type "H-Wide Flange Beams:HE100B" | names: "H-Wide Flange Beams:HE100B:1242364", "H-Wide Flange Beams:HE100B:1242444" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1244428" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1247338" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          22 x IFCBEAM | type IFCBEAMTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1248236", "L-Angles:CAE50x5:1248476", "L-Angles:CAE50x5:1248527" (+19 more) | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Gradil 50mm" | object type "Floor:Gradil 50mm" | FLOOR | names: "Floor:Gradil 50mm:1248585" | material: layers "Floor:Gradil 50mm" ("Betão armado C25/30" 0.050000000000000003) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Circular Hollow Sections:TRON50x2.5" | object type "Circular Hollow Sections:TRON50x2.5" | names: "Circular Hollow Sections:TRON50x2.5:1251136" | material: "Metal - Steel - 345 MPa" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          3 x IFCMEMBER | type IFCMEMBERTYPE "Circular Hollow Sections:TRON50x2.5" | object type "Circular Hollow Sections:TRON50x2.5" | names: "Circular Hollow Sections:TRON50x2.5:1251328", "Circular Hollow Sections:TRON50x2.5:1251722", "Circular Hollow Sections:TRON50x2.5:1272785" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "Circular Hollow Sections:TRON50x2.5" | object type "Circular Hollow Sections:TRON50x2.5" | names: "Circular Hollow Sections:TRON50x2.5:1251608" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCMEMBER | type IFCMEMBERTYPE "Circular Hollow Sections:TRON50x2.5" | object type "Circular Hollow Sections:TRON50x2.5" | names: "Circular Hollow Sections:TRON50x2.5:1251725", "Circular Hollow Sections:TRON50x2.5:1251729" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257240" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257364" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          1 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1257367" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          3 x IFCMEMBER | type IFCMEMBERTYPE "L-Angles:CAE50x5" | object type "L-Angles:CAE50x5" | names: "L-Angles:CAE50x5:1258126", "L-Angles:CAE50x5:1258232", "L-Angles:CAE50x5:1258235" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCMEMBER | type IFCMEMBERTYPE "Circular Hollow Sections:TRON50x2.5" | object type "Circular Hollow Sections:TRON50x2.5" | names: "Circular Hollow Sections:TRON50x2.5:1273445", "Circular Hollow Sections:TRON50x2.5:1273570" | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Model Text:600mm Arial" | object type "Model Text:600mm Arial" | names: "Model Text:600mm Arial:1311177", "Model Text:600mm Arial:1321396" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Coberto 2:Coberto 2" | object type "Coberto 2:Coberto 2" | names: "Coberto 2:Coberto 2:1316693" | material: "Default Form" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCRAILING | type IFCRAILINGTYPE "Railing:1100mm" | object type "Railing:1100mm" | names: "Railing:1100mm:1248629", "Railing:1100mm:1248936" | material: materials ("Metal - Stainless Steel,Polished", "<Unnamed>") | property sets: Pset_QuantityTakeOff, Pset_RailingCommon
          1 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Beam System:Structural Framing System:1316889" | parts: 7 IFCBEAM | property sets: Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Piso 3" | long name "Piso 3" | object type "Level:8mm Head" | elevation 9.5
        contains 1 element
          1 x IFCSLAB | type IFCSLABTYPE "Floor:Generic Floor - 400mm" | object type "Floor:Generic Floor - 400mm" | FLOOR | names: "Floor:Generic Floor - 400mm:1169461" | material: layers "Floor:Generic Floor - 400mm" ("Default Floor" 0.40000000000000002) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon

Types
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 6 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 6 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 4 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCWALLTYPE "Basic Wall:20 cm" | STANDARD | 23 occurrences | material: layers "Basic Wall:20 cm" ("Betão armado C25/30" 0.20000000000000001) | property sets: Pset_WallCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCSLABTYPE "Floor:Generic 200mm" | FLOOR | 2 occurrences | material: layers "Floor:Generic 200mm" ("Betão armado C25/30" 0.20000000000000001) | property sets: Pset_SlabCommon
  IFCSLABTYPE "Floor:Generic Floor - 400mm" | FLOOR | 2 occurrences | material: layers "Floor:Generic Floor - 400mm" ("Default Floor" 0.40000000000000002)
  IFCCOLUMNTYPE "Concrete Round:300mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:300mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:300mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:300mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:300mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:25 x 20cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCTYPEPRODUCT "Assembled Stair:escadas de acesso ao passadiço 2" | 2 occurrences
  IFCBEAMTYPE "U-Channels:UPN80" | BEAM | 24 occurrences | property sets: Pset_BeamCommon
  IFCCURTAINWALLTYPE "Curtain Wall:Curtain Wall" | 1 occurrence
  IFCWALLTYPE "Basic Wall:15 cm" | STANDARD | 3 occurrences | material: layers "Basic Wall:15 cm" ("Betão armado C25/30" 0.14999999999999997) | property sets: Pset_WallCommon
  IFCWALLTYPE "Basic Wall:Generic - 400mm" | STANDARD | 1 occurrence | material: layers "Basic Wall:Generic - 400mm" ("Parede Branca" 0.40000000000000002) | property sets: Pset_WallCommon
  IFCMEMBERTYPE "U-Channels:UPN100" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "U-Channels:UPN80" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "U-Channels:UPN80" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "U-Channels:UPN100" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 13 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 6 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 6 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCSLABTYPE "Foundation Slab:200mm Foundation Slab" | BASESLAB | 1 occurrence | material: layers "Foundation Slab:200mm Foundation Slab" ("Concrete, Cast-in-Place gray" 0.20000000000000001) | property sets: Pset_SlabCommon
  IFCCOLUMNTYPE "M_Concrete-Rectangular-Column:44 x 44 cm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 2:Generic Models 2" | 1 occurrence | material: "<Unnamed>"
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCSLABTYPE "Foundation Slab:300mm Foundation Slab" | BASESLAB | 2 occurrences | material: layers "Foundation Slab:300mm Foundation Slab" ("Concrete, Cast-in-Place gray" 0.30000000000000004) | property sets: Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:600mm Arial" | 9 occurrences
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "Concrete Round:360mm" | COLUMN | 1 occurrence | material: "Concrete, Cast-in-Place gray" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "IPE-Column:IPE200" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "IPE-Column:IPE200" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "IPE-Column:IPE200" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCPIPESEGMENTTYPE "Pipe Types:Default" | 1 occurrence
  IFCPIPEFITTINGTYPE "M_Elbow - Welded - Generic:Standard" | 5 occurrences | material: "<Unnamed>" | property sets: Pset_DuctConnection, Pset_PipeConnection
  IFCPIPESEGMENTTYPE "Pipe Types:Standard" | 5 occurrences
  IFCBEAMTYPE "IPE-Beams:IPE120" | BEAM | 13 occurrences | property sets: Pset_BeamCommon
  IFCBEAMTYPE "H-Wide Flange Beams:HE120B" | 25 occurrences | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 13 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 3 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 2 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBUILDINGELEMENTPROXYTYPE "Mass 3:Mass 3" | 1 occurrence | material: "Default Form"
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "H-Wide Flange Beams:HE120B" | JOIST | 13 occurrences | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "H-Wide Flange Beams:HE120B" | PURLIN | 2 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBEAMTYPE "U-Channels:UPN100" | 2 occurrences | property sets: Pset_BeamCommon
  IFCBEAMTYPE "U-Channels:UPN100" | JOIST | 2 occurrences | property sets: Pset_BeamCommon
  IFCSLABTYPE "Floor:Gradil 50mm" | FLOOR | 3 occurrences | material: layers "Floor:Gradil 50mm" ("Betão armado C25/30" 0.050000000000000003) | property sets: Pset_SlabCommon
  IFCMEMBERTYPE "U-Channels:UPN80" | BRACE | 7 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "U-Channels:UPN80" | PURLIN | 3 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "U-Channels:UPN160" | BRACE | 2 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBUILDINGELEMENTPROXYTYPE "Condensadores:Condensadores" | 1 occurrence | material: "<Unnamed>"
  IFCBUILDINGELEMENTPROXYTYPE "Condensadores1:Condensadores" | 1 occurrence | material: "<Unnamed>"
  IFCMEMBERTYPE "U-Channels:UPN80" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBUILDINGELEMENTPROXYTYPE "Model Text:60 mm" | 2 occurrences
  IFCBEAMTYPE "U-Channels:UPN80" | JOIST | 1 occurrence | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 2 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBUILDINGELEMENTPROXYTYPE "Coberto Nova Parede:Coberto Nova Parede" | 1 occurrence | material: "<Unnamed>"
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 3:Generic Models 3" | 1 occurrence | material: "<Unnamed>"
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 6 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "H-Wide Flange-Column:HE120B" | COLUMN | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_ColumnCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBEAMTYPE "IPE-Beams:IPE120" | 2 occurrences | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBEAMTYPE "U-Channels:UPN60" | BEAM | 2 occurrences | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1:Generic Models 1" | 1 occurrence | material: "<Unnamed>"
  IFCBUILDINGELEMENTPROXYTYPE "Coletor Principal Retorno v1:Coletor Principal Retorno v1" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Coletor Principal Envio:Coletor Principal Envio" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Mass 4:Mass 4" | 1 occurrence | material: "Default Form"
  IFCMEMBERTYPE "IPE-Beams:IPE80" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "IPE-Beams:IPE80" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE80x8" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBEAMTYPE "IPE-Beams:IPE100" | BEAM | 7 occurrences | property sets: Pset_BeamCommon
  IFCBEAMTYPE "U-Channels:UPN100" | BEAM | 4 occurrences | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "Mass 5:Mass 5" | 1 occurrence | material: "Default Form"
  IFCBUILDINGELEMENTPROXYTYPE "Mass 7:Mass 7" | 1 occurrence | material: "Default Form"
  IFCMEMBERTYPE "IPE-Beams:IPE80" | BRACE | 2 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "IPE-Beams:IPE80" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "IPE-Beams:IPE80" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBEAMTYPE "IPE-Beams:IPE100" | JOIST | 2 occurrences | property sets: Pset_BeamCommon
  IFCBEAMTYPE "U-Channels:UPN120" | BEAM | 2 occurrences | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "IPE-Beams:IPE120" | PURLIN | 3 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBEAMTYPE "H-Wide Flange Beams:HE100B" | BEAM | 2 occurrences | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBEAMTYPE "L-Angles:CAE50x5" | BEAM | 22 occurrences | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Circular Hollow Sections:TRON50x2.5" | BEAM | 1 occurrence | property sets: Pset_BeamCommon
  IFCMEMBERTYPE "Circular Hollow Sections:TRON50x2.5" | BRACE | 3 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "Circular Hollow Sections:TRON50x2.5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "Circular Hollow Sections:TRON50x2.5" | BRACE | 2 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "L-Angles:CAE50x5" | BRACE | 1 occurrence | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCMEMBERTYPE "Circular Hollow Sections:TRON50x2.5" | BRACE | 2 occurrences | material: "Metal - Steel - 345 MPa" | property sets: Pset_MemberCommon
  IFCBUILDINGELEMENTPROXYTYPE "Coberto 2:Coberto 2" | 1 occurrence | material: "Default Form"
  IFCRAILINGTYPE "Railing:1100mm" | 2 occurrences

Property sets
  Pset_ColumnCommon | properties | on 25 objects (25 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HE120B" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 8 objects (8 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "44 x 44 cm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 6 objects (6 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "360mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 6 objects (6 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "360mm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 5 objects (5 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "300mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 4 objects (4 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HE120B" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon | properties | on 3 objects (3 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "44 x 44 cm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HE120B" (IFCIDENTIFIER)
    Slope = 89.91538040989353 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Pset_ColumnCommon: 9 more contents on 8 objects not shown
  Pset_QuantityTakeOff | properties | on 75 objects (38 IFCBEAM, 35 IFCCOLUMN, 2 IFCMEMBER)
    Reference = "HE120B" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 73 objects (51 IFCMEMBER, 22 IFCBEAM)
    Reference = "CAE50x5" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 42 objects (42 IFCMEMBER)
    Reference = "CAE80x8" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 39 objects (39 IFCPLATE)
    Reference = "-" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 38 objects (25 IFCBEAM, 13 IFCMEMBER)
    Reference = "UPN80" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 25 objects (22 IFCBEAM, 3 IFCMEMBER)
    Reference = "IPE120" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 24 objects (21 IFCWALLSTANDARDCASE, 2 IFCWALL, 1 IFCOPENINGELEMENT)
    Reference = "20 cm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 13 objects (13 IFCBEAM)
    Reference = "IPE100" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 40 more contents on 133 objects not shown
  Pset_ReinforcementBarPitchOfColumn | properties | on 35 objects (35 IFCCOLUMN)
    Reference = "HE120B" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 12 objects (12 IFCCOLUMN)
    Reference = "360mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 11 objects (11 IFCCOLUMN)
    Reference = "44 x 44 cm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 5 objects (5 IFCCOLUMN)
    Reference = "300mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 3 objects (3 IFCCOLUMN)
    Reference = "IPE200" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 1 object (1 IFCCOLUMN)
    Reference = "25 x 20cm" (IFCLABEL)
  Pset_BeamCommon | properties | on 22 objects (22 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "CAE50x5" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 0.80000000000000004 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HE120B" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 3.4000000000000004 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 5 objects (5 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "IPE100" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 5.2400000000000002 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HE120B" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 2.4009999999999998 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "UPN80" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 9.5389999999999997 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "UPN80" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6.080000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HE120B" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 2.5939999999999999 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HE120B" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 2.7000000000000002 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon: 72 more contents on 88 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 38 objects (38 IFCBEAM)
    Reference = "HE120B" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 25 objects (25 IFCBEAM)
    Reference = "UPN80" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 22 objects (22 IFCBEAM)
    Reference = "CAE50x5" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 22 objects (22 IFCBEAM)
    Reference = "IPE120" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 13 objects (13 IFCBEAM)
    Reference = "IPE100" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 8 objects (8 IFCBEAM)
    Reference = "UPN100" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 5 objects (5 IFCBEAM)
    Reference = "IPE80" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 2 objects (2 IFCBEAM)
    Reference = "UPN60" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam: 3 more contents on 5 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 3 objects (3 IFCSLAB)
    Reference = "Gradil 50mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Generic Floor - 400mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Generic 200mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "300mm Foundation Slab" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "200mm Foundation Slab" (IFCLABEL)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Gradil 50mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic Floor - 400mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic 200mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "300mm Foundation Slab" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "200mm Foundation Slab" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 type objects
    ThermalTransmittance = 5.2300000000000004 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 type object
    ThermalTransmittance = 3.4866666666666668 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 type object
    ThermalTransmittance = 20.920000000000002 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ReinforcementBarPitchOfWall | properties | on 23 objects (21 IFCWALLSTANDARDCASE, 2 IFCWALL)
    Reference = "20 cm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    Reference = "15 cm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Reference = "Generic - 400mm" (IFCLABEL)
  Pset_WallCommon | properties | on 15 objects (14 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "20 cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 8 objects (7 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "20 cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "15 cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "15 cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Generic - 400mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 type object
    ThermalTransmittance = 5.2300000000000004 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    ThermalTransmittance = 6.9733333333333345 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    ThermalTransmittance = 3.25 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "20 cm" (IFCIDENTIFIER)
  Pset_MemberCommon | properties | on 18 objects (18 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "CAE80x8" (IFCIDENTIFIER)
    Slope = 45. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1.6130000000000002 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 16 objects (16 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "CAE50x5" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 0.80000000000000004 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 8 objects (8 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "UPN80" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1.02 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 7 objects (7 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "TRON50x2.5" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1.8 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 6 objects (6 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "CAE50x5" (IFCIDENTIFIER)
    Slope = 60.077870143936458 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1.6040000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 6 objects (6 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "CAE50x5" (IFCIDENTIFIER)
    Slope = 60.077870143936551 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1.6040000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 3 objects (3 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "CAE80x8" (IFCIDENTIFIER)
    Slope = 45.294685466643806 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1.603 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon | properties | on 3 objects (3 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "UPN80" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 2.4000000000000004 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_MemberCommon: 53 more contents on 62 objects not shown
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 15. (IFCCOUNTMEASURE)
    NumberOfTreads = 15. (IFCCOUNTMEASURE)
    Reference = "escadas de acesso ao passadiço 2" (IFCIDENTIFIER)
    RiserHeight = 0.24999999999999997 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.20000000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 4. (IFCCOUNTMEASURE)
    NumberOfTreads = 4. (IFCCOUNTMEASURE)
    Reference = "escadas de acesso ao passadiço 2" (IFCIDENTIFIER)
    RiserHeight = 0.25000000000000017 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.24999999999999997 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 15. (IFCCOUNTMEASURE)
    NumberOfTreads = 15. (IFCCOUNTMEASURE)
    Reference = "Patamar escadas" (IFCIDENTIFIER)
    RiserHeight = 0.24999999999999997 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.20000000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.20000000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.20000000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 1.3123359580052494 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [METRE]
    NumberOfRiser = 4. (IFCCOUNTMEASURE)
    NumberOfTreads = 4. (IFCCOUNTMEASURE)
    Reference = "Patamar escadas" (IFCIDENTIFIER)
    RiserHeight = 0.25000000000000017 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLength = 0.24999999999999997 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtInnerSide = 0.24999999999999997 (IFCPOSITIVELENGTHMEASURE) [METRE]
    TreadLengthAtOffset = 0.24999999999999997 (IFCPOSITIVELENGTHMEASURE) [METRE]
    WalkingLineOffset = 1.3123359580052494 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BuildingElementProxyCommon | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Reference = "600mm Arial" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Condensadores" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "60 mm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Generic Models 2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Coberto Nova Parede" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Mass 3" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Generic Models 3" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 6 more contents on 6 objects not shown
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Curtain Wall" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 39 objects (39 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "-" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 10 objects (5 IFCFLOWFITTING, 5 IFCFLOWSEGMENT)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWSEGMENT)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_DuctConnection | properties | on 6 objects (6 IFCFLOWSEGMENT) | on 1 type object
    ConnectionType = ["Generic"] (IFCTEXT)
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 2.5368049567083593 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 1.2389983823706645 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 3.5371374041234218 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 5.4944856227907781 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 0.83713740412343474 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 2.096514377209227 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 5.9497290199255675 (IFCLENGTHMEASURE) [METRE]
    Length = 2.5368049567083593 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 8.5905739766339266 (IFCLENGTHMEASURE) [METRE]
    Length = 1.2389983823706645 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 8.5905739766339249 (IFCLENGTHMEASURE) [METRE]
    Length = 3.5371374041234218 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 8.5905739766339266 (IFCLENGTHMEASURE) [METRE]
    Length = 5.4944856227907781 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 8.5905739766339266 (IFCLENGTHMEASURE) [METRE]
    Length = 0.83713740412343474 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    InvertElevation = 8.5905739766339266 (IFCLENGTHMEASURE) [METRE]
    Length = 2.096514377209227 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeConnection | properties | on 6 objects (6 IFCFLOWSEGMENT) | on 1 type object
    ConnectionType = ["Generic"] (IFCLABEL)
  Pset_PipeFittingTypeCommon | properties | on 5 objects (5 IFCFLOWFITTING)
    NominalDiameter = [0.20000000000000001] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_RailingCommon | properties | on 6 objects (6 IFCRAILING)
    Height = 1.1000000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1100mm" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 0 IFC" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 0.1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 2" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Coberto 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Coberto 2" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 2.3" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 3" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 8 objects (8 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 0 IFC" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 0.1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 2" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Coberto 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Coberto 2" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 2.3" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Piso 3" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 8 (IFCINTEGER)