IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "RevitIdentifiers [ContentGUID: e5d5eb5b-6f28-4927-98f9-6b086fe0b811, VersionGUID: a5a5a8b3-2111-494f-bfbf-36809655a3a7, NumberOfSaves: 56]"
Description: "CoordinateReference [CoordinateBase: Project Base Point, ProjectSite: Internal]"
Description: "ExchangeRequirement [Architecture]"
File name: "STR - Test Project - R23.ifc"
Time stamp: "2025-02-28T09:33:16+01:00"
Preprocessor: "ODA SDAI 24.12"
Originating system: "Autodesk Revit 25.4.0.32 (ENU) - IFC 25.4.0.32"
Application: "Autodesk Revit 2025 (ENU)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ENU)"

People and organizations
  Person "RVIENG" of Organization (no name given)
  Owner history of Person "RVIENG" of Organization (no name given) | application "Autodesk Revit 2025 (ENU)" version "2025" identifier "Revit" by Organization "Autodesk Revit 2025 (ENU)" | change NOCHANGE | created 1740731586 (2025-02-28T08:33:06Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PRESSUREUNIT: PASCAL
  MASSDENSITYUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  USERDEFINED: derived "Electrical Resistivity"
  MODULUSOFELASTICITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  THERMALCONDUCTANCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.804504″ | longitude -71° 1′ 58.789672″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "STR 01" | long name "STR 01" | object type "Level:1/4" Head" | elevation 0.
        contains 18 elements
          15 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCGRID | names: "Default Grid"
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W10X49" | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn, Qto_ColumnBaseQuantities, ProfileProperties
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W Shapes:W12X26:595507" | descriptions: "BP{DE0DB478-336E-4445-B220-45966B53C6E2}" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 02" | long name "STR 02" | object type "Level:1/4" Head" | elevation 9.8750000000018385
        contains 65 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCSLAB | type IFCSLABTYPE "72" x 48" x 18"" | object type "Footing-Rectangular:72" x 48" x 18"" | BASESLAB | names: "72" x 48" x 18"" | descriptions: "STRUCTURAL FOUNDATIONS" | material: "CE - 03 31 00 - CSC00 - CAST IN PLACE STRUCTURAL CONCRETE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon, Qto_SlabBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "STR 03" | long name "STR 03" | object type "Level:1/4" Head" | elevation 19.875
        contains 76 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:635799" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635800", "W Shapes:W12X26:635803" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635801" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635802" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 04" | long name "STR 04" | object type "Level:1/4" Head" | elevation 29.875
        contains 76 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:635828" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635829", "W Shapes:W12X26:635832" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635830" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635831" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 05" | long name "STR 05" | object type "Level:1/4" Head" | elevation 39.875
        contains 76 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:635857" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635858", "W Shapes:W12X26:635861" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635859" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635860" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 06" | long name "STR 06" | object type "Level:1/4" Head" | elevation 49.875
        contains 76 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:635886" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635887", "W Shapes:W12X26:635890" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635888" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635889" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 07" | long name "STR 07" | object type "Level:1/4" Head" | elevation 59.875
        contains 77 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:634237" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:634308", "W Shapes:W12X26:634398" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:634340" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:634396" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:634397" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 08" | long name "STR 08" | object type "Level:1/4" Head" | elevation 69.875
        contains 76 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:635770" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635771", "W Shapes:W12X26:635774" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635772" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635773" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 25 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 09" | long name "STR 09" | object type "Level:1/4" Head" | elevation 79.875
        contains 76 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:635738" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635739", "W Shapes:W12X26:635742" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635740" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635741" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
      IFCBUILDINGSTOREY "STR 10" | long name "STR 10" | object type "Level:1/4" Head" | elevation 89.875
        contains 76 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:635915" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635916", "W Shapes:W12X26:635919" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635917" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635918" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 11" | long name "STR 11" | object type "Level:1/4" Head" | elevation 99.875
        contains 76 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:635944" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635945", "W Shapes:W12X26:635948" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635946" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635947" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 12" | long name "STR 12" | object type "Level:1/4" Head" | elevation 109.875
        contains 76 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:635973" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635974", "W Shapes:W12X26:635977" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635975" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:635976" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 25 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 13" | long name "STR 13" | object type "Level:1/4" Head" | elevation 119.875
        contains 76 elements
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:636002" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:636003", "W Shapes:W12X26:636006" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:636004" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:636005" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 14" | long name "STR 14" | object type "Level:1/4" Head" | elevation 129.875
        contains 64 elements
          3 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          4 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "W10X49" | object type "W Shapes-Column:W10X49" | COLUMN | names: "W10X49" | descriptions: "STRUCTURAL COLUMN" | material: "Steel ASTM A992" | property sets: Qto_ColumnBaseQuantities, Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          6 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          7 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26", "W Shapes:W12X26:636031" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          2 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:636032", "W Shapes:W12X26:636035" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:636033" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W Shapes:W12X26:636034" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W Shapes:W12X26" | JOIST | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          8 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Framing System" | descriptions: "BEAM SYSTEM" | parts: 24 IFCBEAM | property sets: Pset_ElementAssemblyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCGRID | names: "Default Grid"
          1 x IFCBEAM | type IFCBEAMTYPE "W12X26" | object type "W12X26" | names: "W12X26" | descriptions: "STRUCTURAL BEAM 01" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities, ProfileProperties
      IFCBUILDINGSTOREY "STR 15" | long name "STR 15" | object type "Level:1/4" Head" | elevation 139.87499999999997
        contains 7 elements
          1 x IFCBEAM | type IFCBEAMTYPE "W14X30" | object type "W Shapes:W14X30" | BEAM | names: "W14X30" | descriptions: "STRUCTURAL BEAM 02" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W14X30" | object type "W Shapes:W14X30" | BEAM | names: "W14X30" | descriptions: "STRUCTURAL BEAM 02" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W14X30" | object type "W Shapes:W14X30" | BEAM | names: "W14X30" | descriptions: "STRUCTURAL BEAM 02" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W14X30" | object type "W Shapes:W14X30" | BEAM | names: "W14X30" | descriptions: "STRUCTURAL BEAM 02" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W14X30" | object type "W Shapes:W14X30" | BEAM | names: "W14X30" | descriptions: "STRUCTURAL BEAM 02" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCBEAM | type IFCBEAMTYPE "W14X30" | object type "W Shapes:W14X30" | BEAM | names: "W14X30" | descriptions: "STRUCTURAL BEAM 02" | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam, Qto_BeamBaseQuantities
          1 x IFCGRID | names: "Default Grid"

Types
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | BEAM | 12 occurrences | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 88 occurrences | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 97 occurrences | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 8 occurrences | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCSLABTYPE "72" x 48" x 18"" | BASESLAB | 16 occurrences | material: "CE - 03 31 00 - CSC00 - CAST IN PLACE STRUCTURAL CONCRETE" | property sets: Pset_ReinforcementBarPitchOfSlab | description "STRUCTURAL FOUNDATIONS"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 91 occurrences | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 72 occurrences | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 72 occurrences | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 84 occurrences | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 24 occurrences | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 16 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 3 occurrences | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 7 occurrences | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCCOLUMNTYPE "W10X49" | COLUMN | 4 occurrences | material: "Steel ASTM A992" | property sets: Pset_ColumnCommon, Pset_ReinforcementBarPitchOfColumn | description "STRUCTURAL COLUMN"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W12X26" | JOIST | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 01"
  IFCBEAMTYPE "W14X30" | BEAM | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 02"
  IFCBEAMTYPE "W14X30" | BEAM | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 02"
  IFCBEAMTYPE "W14X30" | BEAM | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 02"
  IFCBEAMTYPE "W14X30" | BEAM | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 02"
  IFCBEAMTYPE "W14X30" | BEAM | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 02"
  IFCBEAMTYPE "W14X30" | BEAM | 1 occurrence | material: "Steel ASTM A992" | property sets: Pset_BeamCommon, Pset_ReinforcementBarPitchOfBeam | description "STRUCTURAL BEAM 02"

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Qto_ColumnBaseQuantities | quantities | on 176 objects (176 IFCCOLUMN)
    CrossSectionArea = 0.10023600726077032 [SQUARE FOOT (conversion based)]
    GrossVolume = 1.0023600726077033 [CUBIC FOOT (conversion based)]
    Length = 10. [FOOT (conversion based)]
    NetVolume = 1.0023834963736624 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 48.717993877991475 [SQUARE FOOT (conversion based)]
  Qto_ColumnBaseQuantities | quantities | on 16 objects (16 IFCCOLUMN)
    CrossSectionArea = 0.10023600726077032 [SQUARE FOOT (conversion based)]
    GrossVolume = 1.002360072607519 [CUBIC FOOT (conversion based)]
    Length = 9.9999999999981615 [FOOT (conversion based)]
    NetVolume = 1.0023834963734788 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 48.717993877982522 [SQUARE FOOT (conversion based)]
  Qto_ColumnBaseQuantities | quantities | on 15 objects (15 IFCCOLUMN)
    CrossSectionArea = 0.10023600726077032 [SQUARE FOOT (conversion based)]
    GrossVolume = 0.98983057170029121 [CUBIC FOOT (conversion based)]
    Length = 9.8750000000018385 [FOOT (conversion based)]
    NetVolume = 0.98985370266917605 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 48.109018954525538 [SQUARE FOOT (conversion based)]
  Qto_ColumnBaseQuantities | quantities | on 4 objects (4 IFCCOLUMN)
    CrossSectionArea = 0.10023600726077032 [SQUARE FOOT (conversion based)]
    GrossVolume = 1.0023600726077004 [CUBIC FOOT (conversion based)]
    Length = 9.9999999999999716 [FOOT (conversion based)]
    NetVolume = 1.0023834963736609 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 48.71799387799134 [SQUARE FOOT (conversion based)]
  Qto_ColumnBaseQuantities | quantities | on 1 object (1 IFCCOLUMN)
    Length = 9.8750000000018385 [FOOT (conversion based)]
    NetSurfaceArea = 48.309511563612432 [SQUARE FOOT (conversion based)]
    NetVolume = 0.98985370266917494 [CUBIC FOOT (conversion based)]
  Pset_ColumnCommon | properties | on 212 objects (212 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W10X49" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 14 type objects
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_EnvironmentalImpactIndicators | properties | on 952 objects (952 IFCBEAM)
    Reference = "W12X26" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 212 objects (212 IFCCOLUMN)
    Reference = "W10X49" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 104 objects (104 IFCELEMENTASSEMBLY)
    Reference = "Structural Framing System" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 16 objects (16 IFCSLAB)
    Reference = "72" x 48" x 18"" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 6 objects (6 IFCBEAM)
    Reference = "W14X30" (IFCIDENTIFIER)
  Pset_ReinforcementBarPitchOfColumn | properties | on 212 objects (212 IFCCOLUMN)
    Reference = "W10X49" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 14 type objects
    Description = "STRUCTURAL COLUMN" (IFCTEXT)
  Pset_BeamCommon | properties | on 448 objects (448 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W12X26" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 13. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 192 objects (192 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W12X26" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 5. (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 141 objects (141 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W12X26" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 13.123359580052494 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 49 objects (49 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W12X26" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 12.753280839894707 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 24 objects (24 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W12X26" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 13.123359580052492 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 22 objects (22 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W12X26" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 12.753280839895101 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 21 objects (21 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W12X26" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 13.123359580052496 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 12 objects (12 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W12X26" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 13.123359580052488 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon: 22 more contents on 49 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 952 objects (952 IFCBEAM)
    Reference = "W12X26" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 6 objects (6 IFCBEAM)
    Reference = "W14X30" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 91 type objects
    Description = "STRUCTURAL BEAM 01" (IFCTEXT)
  Pset_ReinforcementBarPitchOfBeam | properties | on 6 type objects
    Description = "STRUCTURAL BEAM 02" (IFCTEXT)
  Qto_BeamBaseQuantities | quantities | on 23 objects (23 IFCBEAM)
    CrossSectionArea = 0.053062215117476975 [SQUARE FOOT (conversion based)]
    GrossSurfaceArea = 51.037789395447561 [SQUARE FOOT (conversion based)]
    GrossVolume = 0.6566891305913618 [CUBIC FOOT (conversion based)]
    Length = 13. [FOOT (conversion based)]
    NetSurfaceArea = 51.037789395447547 [SQUARE FOOT (conversion based)]
    NetVolume = 0.65668127098240714 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 50.931664965212605 [SQUARE FOOT (conversion based)]
  Qto_BeamBaseQuantities | quantities | on 12 objects (12 IFCBEAM)
    CrossSectionArea = 0.053062215117476975 [SQUARE FOOT (conversion based)]
    GrossSurfaceArea = 51.037789395447561 [SQUARE FOOT (conversion based)]
    GrossVolume = 0.6566891305913618 [CUBIC FOOT (conversion based)]
    Length = 13. [FOOT (conversion based)]
    NetSurfaceArea = 51.037789395447547 [SQUARE FOOT (conversion based)]
    NetVolume = 0.65668127098242313 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 50.931664965212605 [SQUARE FOOT (conversion based)]
  Qto_BeamBaseQuantities | quantities | on 12 objects (12 IFCBEAM)
    CrossSectionArea = 0.053062215117476975 [SQUARE FOOT (conversion based)]
    GrossSurfaceArea = 51.037789395447561 [SQUARE FOOT (conversion based)]
    GrossVolume = 0.6566891305913618 [CUBIC FOOT (conversion based)]
    Length = 12.999999999999687 [FOOT (conversion based)]
    NetSurfaceArea = 51.037789395447547 [SQUARE FOOT (conversion based)]
    NetVolume = 0.65668127098239371 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 50.931664965212605 [SQUARE FOOT (conversion based)]
  Qto_BeamBaseQuantities | quantities | on 12 objects (12 IFCBEAM)
    CrossSectionArea = 0.053062215117476975 [SQUARE FOOT (conversion based)]
    GrossSurfaceArea = 51.037789395447561 [SQUARE FOOT (conversion based)]
    GrossVolume = 0.6566891305913618 [CUBIC FOOT (conversion based)]
    Length = 12.999999999999689 [FOOT (conversion based)]
    NetSurfaceArea = 51.037789395447547 [SQUARE FOOT (conversion based)]
    NetVolume = 0.65668127098240714 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 50.931664965212605 [SQUARE FOOT (conversion based)]
  Qto_BeamBaseQuantities | quantities | on 12 objects (12 IFCBEAM)
    CrossSectionArea = 0.053062215117476975 [SQUARE FOOT (conversion based)]
    GrossSurfaceArea = 49.834031102889867 [SQUARE FOOT (conversion based)]
    GrossVolume = 0.64116843266951329 [CUBIC FOOT (conversion based)]
    Length = 13.123359580052494 [FOOT (conversion based)]
    NetSurfaceArea = 49.834031102889845 [SQUARE FOOT (conversion based)]
    NetVolume = 0.64116075882062484 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 49.72790667265491 [SQUARE FOOT (conversion based)]
  Qto_BeamBaseQuantities | quantities | on 12 objects (12 IFCBEAM)
    CrossSectionArea = 0.053062215117476975 [SQUARE FOOT (conversion based)]
    GrossSurfaceArea = 49.834031102889831 [SQUARE FOOT (conversion based)]
    GrossVolume = 0.64116843266951296 [CUBIC FOOT (conversion based)]
    Length = 13.123359580052494 [FOOT (conversion based)]
    NetSurfaceArea = 49.834031102889824 [SQUARE FOOT (conversion based)]
    NetVolume = 0.64116075882061119 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 49.727906672654875 [SQUARE FOOT (conversion based)]
  Qto_BeamBaseQuantities | quantities | on 12 objects (12 IFCBEAM)
    CrossSectionArea = 0.053062215117477017 [SQUARE FOOT (conversion based)]
    GrossSurfaceArea = 19.90983457376938 [SQUARE FOOT (conversion based)]
    GrossVolume = 0.25533980099656212 [CUBIC FOOT (conversion based)]
    Length = 5.0000000000000009 [FOOT (conversion based)]
    NetSurfaceArea = 19.909834573769377 [SQUARE FOOT (conversion based)]
    NetVolume = 0.25533674495239106 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 19.803710143534428 [SQUARE FOOT (conversion based)]
  Qto_BeamBaseQuantities | quantities | on 11 objects (11 IFCBEAM)
    CrossSectionArea = 0.053062215117476975 [SQUARE FOOT (conversion based)]
    GrossSurfaceArea = 51.037789395447561 [SQUARE FOOT (conversion based)]
    GrossVolume = 0.6566891305913618 [CUBIC FOOT (conversion based)]
    Length = 13.000000000000007 [FOOT (conversion based)]
    NetSurfaceArea = 51.037789395447547 [SQUARE FOOT (conversion based)]
    NetVolume = 0.65668127098239393 [CUBIC FOOT (conversion based)]
    OuterSurfaceArea = 50.931664965212605 [SQUARE FOOT (conversion based)]
  Qto_BeamBaseQuantities: 320 more contents on 852 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 16 objects (16 IFCSLAB)
    Reference = "72" x 48" x 18"" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 type object
    Description = "STRUCTURAL FOUNDATIONS" (IFCTEXT)
  Pset_SlabCommon | properties | on 16 objects (16 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "72" x 48" x 18"" (IFCIDENTIFIER)
  Qto_SlabBaseQuantities | quantities | on 4 objects (4 IFCSLAB)
    Depth = 1.5 [FOOT (conversion based)]
    GrossArea = 23.999999999999996 [SQUARE FOOT (conversion based)]
    GrossVolume = 35.999999999999993 [CUBIC FOOT (conversion based)]
    Length = 6. [FOOT (conversion based)]
    NetArea = 23.999999999999993 [SQUARE FOOT (conversion based)]
    NetVolume = 35.999999999999986 [CUBIC FOOT (conversion based)]
    Perimeter = 20. [FOOT (conversion based)]
    Width = 4. [FOOT (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 4 objects (4 IFCSLAB)
    Depth = 1.5 [FOOT (conversion based)]
    GrossArea = 24. [SQUARE FOOT (conversion based)]
    GrossVolume = 36. [CUBIC FOOT (conversion based)]
    Length = 6. [FOOT (conversion based)]
    NetArea = 23.999999999999993 [SQUARE FOOT (conversion based)]
    NetVolume = 36.000000000000007 [CUBIC FOOT (conversion based)]
    Perimeter = 20. [FOOT (conversion based)]
    Width = 4. [FOOT (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 4 objects (4 IFCSLAB)
    Depth = 1.5 [FOOT (conversion based)]
    GrossArea = 23.999999999999989 [SQUARE FOOT (conversion based)]
    GrossVolume = 35.999999999999986 [CUBIC FOOT (conversion based)]
    Length = 6. [FOOT (conversion based)]
    NetArea = 23.999999999999993 [SQUARE FOOT (conversion based)]
    NetVolume = 35.999999999999986 [CUBIC FOOT (conversion based)]
    Perimeter = 19.999999999999996 [FOOT (conversion based)]
    Width = 4. [FOOT (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 4 objects (4 IFCSLAB)
    Depth = 1.5 [FOOT (conversion based)]
    GrossArea = 23.999999999999993 [SQUARE FOOT (conversion based)]
    GrossVolume = 35.999999999999986 [CUBIC FOOT (conversion based)]
    Length = 6. [FOOT (conversion based)]
    NetArea = 23.999999999999993 [SQUARE FOOT (conversion based)]
    NetVolume = 35.999999999999993 [CUBIC FOOT (conversion based)]
    Perimeter = 20. [FOOT (conversion based)]
    Width = 4. [FOOT (conversion based)]
  Pset_ElementAssemblyCommon | properties | on 104 objects (104 IFCELEMENTASSEMBLY)
    Reference = "Structural Framing System" (IFCIDENTIFIER)
  ProfileProperties | properties | on 12 objects (12 IFCBEAM)
    Section = "BP{DE0DB478-336E-4445-B220-45966B53C6E2}" (IFCIDENTIFIER)
    SectionFamily = "{DE0DB478-336E-4445-B220-45966B53C6E2}BP" (IFCIDENTIFIER)
  ProfileProperties | properties | on 1 object (1 IFCCOLUMN)
    Section = "BP{17231954-509B-4C6D-8DBB-54610329088A}" (IFCIDENTIFIER)
    SectionFamily = "{DE0DB478-336E-4445-B220-45966B53C6E2}BP" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 15 objects (15 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "1/4" Head" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 15 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)